{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":10,"n_cols":6,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["程序/文档名称","是否为新版本","版本改动","是否需要测试","是否已经测试","测试结果说明"]
["油气回收系统安装包V1.14.61.zip","是","1、增加数据上传南京环保局\n2、按新国标增加严重气液比预报警功能\n3、按新国标增加气体浓度三天预警转报警的功能\n4、为了避免安装升级时误点击多个安装升级的bat批处理文件，仅保留1366*768的批处理文件（\"安装_1366_768.bat\"），且重复点击会提示另一程序正在使用此文件。如果屏幕分辨率是1024*768的则需要在安装升级后再双击另一个bat文件(\"屏幕分辨率是1024_768的则在安装后再双击此文件.bat\")\n5、增加数据上传广东中石化\n6、增加数据上传附件厦门环保局\n7、增加数据上传东莞环保局\n8、增加不同工况下气液比补偿的功能\n9、增加数据上传深圳环保局","是"]
["油气回收在线监控系统安装配置使用更新文档 V2.3.docx","是","1、\t第五部分预报警规则与参数改为新增功能说明，预报警规则改为其中第一点；\n2、\t新增功能说明增加严重气液比预报警、气体浓度预报警","是"]
["广东中石化独立的气液比预警范围统计说明 V1.0.docx","是","新增","可选"]
["加密狗相关问题处理方法 V1.1.docx","否"]
["油气回收在线监控系统数据转移和恢复方法 V1.3.docx","否"]
["360配置与故障排查方法 V1.1","否"]
["油气回收各地区预报警规则与参数列表 V2.1.xlsx","否"]
["部分地区平台的额外配置说明 V2.1","否"]
["加油累计不足5笔规则说明 V1.0.docx"]